This is a simple program that flashes the LEDs on the
Wytec Dragon12 development Rev E board. This board uses a
MC9S12DG256 (a type of 68hc12) processor.

In order to turn on the LED on the rev E board, PJ1 must be programmed as an output and set to low.  

http://www.evbplus.com/
